Boat Traffic Control Plan

**1.0  Description.**  This work shall consist of providing and maintaining a boat traffic control plan as shown on the drawings. The contractor is advised that special sign assemblies and buoys shall be required for the safety and control of boat traffic as well as safety to the contractor.

**2.0  Construction.**

**2.1  Sign Requirements.** All special sign assemblies and buoys shall be anchored to the bottom of the lake as shown on the Missouri Standard Plans for Highway Construction. Each special sign assembly shall be equipped with two (2) flashing light units with amber lens.

The Contractor will be required to furnish, place as shown on the plans, maintain and/or replace these signs and buoys throughout the period of this contract and to remove them when the project is completed. The Contractor shall be required to make any revisions requested by the Missouri State Water Patrol.

**2.2  Placement Requirements.**  As part of the Contractor’s work schedule submittal, a schedule for placement and removal of signs and buoys and an Application for Buoy Permit shall be submitted to the Missouri State Water Patrol. The placement and removal of these signs and buoys shall be subject to the approval of the Water Patrol and the Water Patrol shall be notified thirty (30) days prior to placement or removal of any signs or buoys. If the Contractor restricts boat traffic from more than one work area at a time, there shall be a minimum of 150 feet clear between restricted areas unless otherwise approved by the Water Patrol.

Any barge or working platform that may be used by the Contractor and is left in the work area during the hours of dusk to dawn shall be equipped with a flashing light unit with amber lens on each corner of each barge and/or working platform.

**3.0  Water Patrol Contact.**

The address of the Water Patrol is:

Missouri State Water Patrol

Attn: Capt. Matt Walz

1510 East Elm Street

Jefferson City, Missouri 65101

Telephone: (573) 751-5071

**4.0 Method of Measurement and Basis of Payment.**

All expenses incurred by the Contractor by reason of their compliance with this provision shall be considered completely covered by the unit prices for the following items:

**Item No. Description Unit**

616-10.12 Buoys (BOATS KEEP OUT) Each

616-10.13 Buoys (NO WAKE) Each

616-10.14 Special Sign Assembly (BOATS KEEP OUT) Each